Key Features

It has diopter adjustment function with target priority switch system for measuring overlapping subjects. It Comes with 2 set of rechargeable battery with one charger.

|  |  |
| --- | --- |
| Actual field of view | : 7° |
| Maximum measurement distance(Static target) | : 1100m |
| Minimum measurement distance | : 5m |
| Maximum measurement distance(Moving target) | : 650m |
| Accuracy (Actual distance) | : ±0.5m(5-99m)±1m(100m-1100m) |
| Magnification | : 7x |
| Power source | : CR2 Lithium battery along with automaticpower shutoff function |
| Environment condition | : IP x 4 |
| Laser classification | : Class I |
| Temperature tolerance | : -10oC to +60oC |
| Standard | : ISO |
| Accessories | : Lens cleaning kit, Carry bag and operatingmanual in English/Chinese |