Key Features

It has Spherical lens and prism made of optical glass, multi coated optic. Fold down eyecups and made of rubber. Nitrogen purging and Makrolon housing. Waterproof: 2 hours @1.5 meters depth and also shock resistant: 1.5-meter height in sand. It also capable of range finder illuminated compass (ranging reticle with illuminated compass) and UV protection.

|  |  |
| --- | --- |
| Field of view (at 1000m) | : 132m |
| Lens | : Fully multi-coated |
| Magnification | : 7x |
| Field angle | : 7° |
| Exit pupil diameter | : 7mm |
| Prism | : Porro |
| Eye pupil adjustment | : Yes |
| Body style | : Semi-aromatic thermoplastic |
| Objective diameter | : 50mm |
| Surface treatment | : Rubber |
| Standard | : ISO |
| Accessories | : Carrying case and operating manual inEnglish/Chinese |